Supported Devices & Architectures
=================================

ar71xx-generic
--------------

* 8devices

  - Carambola 2

* ALFA Network

  - AP121
  - AP121F
  - AP121U
  - Hornet-UB
  - Tube2H
  - N2
  - N5

* Allnet

  - ALL0315N

* AVM

  - Fritz!Box 4020 [#avmflash]_
  - Fritz!WLAN Repeater 300E [#avmflash]_
  - Fritz!WLAN Repeater 450E [#avmflash]_

* Buffalo

  - WZR-HP-AG300H / WZR-600DHP
  - WZR-HP-G300NH
  - WZR-HP-G300NH2
  - WZR-HP-G450H

* D-Link

  - DAP-1330 (A1)
  - DIR-505 (A1, A2)
  - DIR-825 (B1)

* GL Innovations

  - GL-AR150
  - GL-AR300M
  - GL-AR750 [#ath10k]_
  - GL-iNet 6408A (v1)
  - GL-iNet 6416A (v1)

* Linksys

  - WRT160NL

* Netgear

  - WNDR3700 (v1, v2, v5)
  - WNDR3800
  - WNDRMAC (v2)

* OCEDO

  - Koala [#ath10k]_

* OpenMesh

  - A40
  - A60
  - MR600 (v1, v2)
  - MR900 (v1, v2)
  - MR1750 (v1, v2) [#ath10k]_
  - OM2P (v1, v2, v4)
  - OM2P-HS (v1, v2, v3, v4)
  - OM2P-LC
  - OM5P
  - OM5P-AN
  - OM5P-AC (v1, v2) [#ath10k]_

* TP-Link

  - Archer C5 (v1) [#ath10k]_
  - Archer C59 (v1) [#80211s]_
  - Archer C7 (v2, v4, v5) [#ath10k]_
  - CPE210 (v1.0, v1.1, v2.0, v3.0)
  - CPE220 (v1.1)
  - CPE510 (v1.0, v1.1)
  - CPE520 (v1.1)
  - RE450 [#ath10k]_
  - TL-WDR3500 (v1)
  - TL-WDR3600 (v1)
  - TL-WDR4300 (v1)
  - TL-WR710N (v1, v2.1)
  - TL-WR810N (v1)
  - TL-WR842N/ND (v1, v2, v3)
  - TL-WR1043N/ND (v1, v2, v3, v4, v5)
  - TL-WR2543N/ND (v1)
  - WBS210 (v1.20)
  - WBS510 (v1.20)

* Ubiquiti

  - Air Gateway
  - Air Gateway LR
  - Air Gateway PRO
  - Air Router
  - Bullet M2/M5
  - Loco M2/M5
  - Loco M2/M5 XW
  - Nanostation M2/M5
  - Nanostation M2/M5 XW
  - Picostation M2
  - Rocket M2/M5
  - Rocket M2/M5 Ti
  - Rocket M2/M5 XW
  - UniFi AC Mesh [#ath10k]_
  - UniFi AC Mesh Pro [#ath10k]_
  - UniFi AP
  - UniFi AP AC Lite [#ath10k]_
  - UniFi AP AC LR [#ath10k]_
  - UniFi AP AC Pro [#ath10k]_
  - UniFi AP LR
  - UniFi AP Pro
  - UniFi AP Outdoor
  - UniFi AP Outdoor+

* Western Digital

  - My Net N600
  - My Net N750

* ZyXEL

  - NBG6616 [#ath10k]_

ar71xx-nand
-----------

* Aerohive

  - HiveAP 121

* Netgear

  - WNDR3700 (v4)
  - WNDR4300 (v1)

* ZyXEL

  - NBG6716 [#ath10k]_

ar71xx-tiny
-----------

* D-Link

  - DIR-615 (C1)

* TP-Link

  - TL-MR13U (v1)
  - TL-MR3020 (v1)
  - TL-MR3040 (v1, v2)
  - TL-MR3220 (v1, v2)
  - TL-MR3420 (v1, v2)
  - TL-WA701N/ND (v1, v2)
  - TL-WA730RE (v1)
  - TL-WA750RE (v1)
  - TL-WA801N/ND (v1, v2, v3)
  - TL-WA830RE (v1, v2)
  - TL-WA850RE (v1)
  - TL-WA860RE (v1)
  - TL-WA901N/ND (v1, v2, v3, v4, v5)
  - TL-WA7210N (v2)
  - TL-WA7510N (v1)
  - TL-WR703N (v1)
  - TL-WR710N (v2)
  - TL-WR740N (v1, v3, v4, v5)
  - TL-WR741N/ND (v1, v2, v4, v5)
  - TL-WR743N/ND (v1, v2)
  - TL-WR840N (v2)
  - TL-WR841N/ND (v3, v5, v7, v8, v9, v10, v11, v12)
  - TL-WR843N/ND (v1)
  - TL-WR940N (v1, v2, v3, v4, v5, v6)
  - TL-WR941ND (v2, v3, v4, v5, v6)

brcm2708-bcm2708
----------------

* RaspberryPi 1

brcm2708-bcm2709
----------------

* RaspberryPi 2


ipq40xx [#80211s]_
------------------

* AVM

  - FRITZ!Box 4040 [#avmflash]_

* GL.iNet

  - GL-B1300

* NETGEAR

  - EX6100v2
  - EX6150v2

* OpenMesh

  - A42
  - A62

* ZyXEL

  - NBG6617
  - WRE6606

mpc85xx-generic
---------------

* TP-Link

  - TL-WDR4900 (v1)

mpc85xx-p1020
---------------

* Aerohive

  - HiveAP 330

ramips-mt7620 [#80211s]_
------------------------

* GL Innovations

  - GL-MT300A
  - GL-MT300N
  - GL-MT750

* Nexx

  - WT3020AD/F/H

ramips-mt7621
-------------

* ASUS

  - RT-AC57U [#80211s]_

* D-Link

  - DIR-860L (B1) [#80211s]_

* Ubiquiti

  - EdgeRouter X
  - EdgeRouter X-SFP

* ZBT

  - WG3526-16M [#80211s]_
  - WG3526-32M [#80211s]_

ramips-mt76x8 [#80211s]_
------------------------

* GL.iNet

  - GL-MT300N v2

* NETGEAR

  - R6120

* TP-Link

  - TL-MR3420 v5
  - TL-WR841N v13
  - Archer C50 v3
  - Archer C50 v4

* VoCore

  - VoCore2

ramips-rt305x [#80211s]_
------------------------

* A5-V11

* D-Link

  - DIR-615 (D1, D2, D3, D4, H1)

* VoCore

  - VoCore (8M, 16M)

sunxi-cortexa7
--------------

* LeMaker

  - Banana Pi M1

x86-generic
-----------

* x86-generic
* x86-virtualbox
* x86-vmware

See also: :doc:`x86`

x86-geode
---------

* x86-geode

See also: :doc:`x86`

x86-64
------

* x86-64-generic
* x86-64-virtualbox
* x86-64-vmware

See also: :doc:`x86`

Footnotes
---------

.. [#ath10k]
  Device uses the ath10k WLAN driver. Images are built for 11s by default unless GLUON_WLAN_MESH
  is set as described in :ref:`getting-started-make-variables`.

.. [#80211s]
  Device or target does not support IBSS. Images are built by default unless
  GLUON_WLAN_MESH is explicitly set to something other than *11s*. Targets that
  are affected as a whole may not be selected for build in this case.

.. [#avmflash]
  For instructions on how to flash AVM devices, visit https://fritzfla.sh
