From: David Bauer <mail@david-bauer.net>
Date: Thu, 9 May 2019 18:01:13 +0200
Subject: ramips: fix R6120 factory image

The factory firmware omits the JFFS2 end-marker while flashing via
web-interface. Add a 64k padding after the marker fixes this problem.

When the end-marker is not present, OpenWRT won't save the overlayfs
after initial flash.

Reported-by: Andreas Ziegler <dev@andreas-ziegler.de>
Signed-off-by: David Bauer <mail@david-bauer.net>

diff --git a/target/linux/ramips/image/mt76x8.mk b/target/linux/ramips/image/mt76x8.mk
index f1bf78e0713a1bc47d4ac384efdac1d08c1bd8bc..a096720b09be18bae450edaab187df8be734fe13 100644
--- a/target/linux/ramips/image/mt76x8.mk
+++ b/target/linux/ramips/image/mt76x8.mk
@@ -118,7 +118,7 @@ define Device/netgear_r6120
   IMAGES += factory.img
   IMAGE/default := append-kernel | pad-to $$$$(BLOCKSIZE)| append-rootfs | pad-rootfs
   IMAGE/sysupgrade.bin := $$(IMAGE/default) | append-metadata | check-size $$$$(IMAGE_SIZE)
-  IMAGE/factory.img := pad-extra 576k | $$(IMAGE/default) | \
+  IMAGE/factory.img := pad-extra 576k | $$(IMAGE/default) | pad-to $$$$(BLOCKSIZE) | \
 	sercom-footer | pad-to 128 | zip R6120.bin | sercom-seal
 endef
 TARGET_DEVICES += netgear_r6120
