From: Adrian Schmutzler <freifunk@adrianschmutzler.de>
Date: Wed, 10 Oct 2018 20:05:53 +0200
Subject: firmware-utils: tplink-safeloader: Add CPE210 v3

Add TP-Link CPE210 v3 to the support list.
It's identical to the v2.

Signed-off-by: Robert Marko <robimarko@gmail.com>
[Use separate definition to prevent cross-updates]
Signed-off-by: Adrian Schmutzler <freifunk@adrianschmutzler.de>

diff --git a/tools/firmware-utils/src/tplink-safeloader.c b/tools/firmware-utils/src/tplink-safeloader.c
index 4b227e1c97b6c5b236dba29dbdd5f0bcd68621cb..de15faf6796c993efc6c2a36b22bb1e978e3be90 100644
--- a/tools/firmware-utils/src/tplink-safeloader.c
+++ b/tools/firmware-utils/src/tplink-safeloader.c
@@ -197,6 +197,42 @@ static struct device_info boards[] = {
 		.last_sysupgrade_partition = "support-list",
 	},
 
+	/** Firmware layout for the CPE210 V3 */
+	{
+		.id     = "CPE210V3",
+		.vendor = "CPE210(TP-LINK|UN|N300-2|00000000):3.0\r\n",
+		.support_list =
+			"SupportList:\r\n"
+			"CPE210(TP-LINK|EU|N300-2|45550000):3.0\r\n"
+			"CPE210(TP-LINK|UN|N300-2|00000000):3.0\r\n"
+			"CPE210(TP-LINK|UN|N300-2):3.0\r\n"
+			"CPE210(TP-LINK|EU|N300-2):3.0\r\n",
+		.support_trail = '\xff',
+		.soft_ver = NULL,
+
+		.partitions = {
+			{"fs-uboot", 0x00000, 0x20000},
+			{"partition-table", 0x20000, 0x02000},
+			{"default-mac", 0x30000, 0x00020},
+			{"product-info", 0x31100, 0x00100},
+			{"device-info", 0x31400, 0x00400},
+			{"signature", 0x32000, 0x00400},
+			{"device-id", 0x33000, 0x00100},
+			{"os-image", 0x40000, 0x1c0000},
+			{"file-system", 0x200000, 0x5b0000},
+			{"soft-version", 0x7b0000, 0x00100},
+			{"support-list", 0x7b1000, 0x01000},
+			{"user-config", 0x7c0000, 0x10000},
+			{"default-config", 0x7d0000, 0x10000},
+			{"log", 0x7e0000, 0x10000},
+			{"radio", 0x7f0000, 0x10000},
+			{NULL, 0, 0}
+		},
+
+		.first_sysupgrade_partition = "os-image",
+		.last_sysupgrade_partition = "support-list",
+	},
+
 	/** Firmware layout for the CPE510/520 */
 	{
 		.id	= "CPE510",
