From: Jan Alexander <jan@nalx.net>
Date: Tue, 31 Mar 2020 21:50:28 +0200
Subject: ath79: enable GL-AR750S NOR variant from master

diff --git a/target/linux/ath79/base-files/etc/board.d/02_network b/target/linux/ath79/base-files/etc/board.d/02_network
index 5dda551caae0429880ee9d5965bfb6797d218e6d..b8fac8816c9a2b2a87a5d1335b41127666afe2e4 100755
--- a/target/linux/ath79/base-files/etc/board.d/02_network
+++ b/target/linux/ath79/base-files/etc/board.d/02_network
@@ -155,7 +155,7 @@ ath79_setup_interfaces()
 	etactica,eg200)
 		ucidef_set_interface_lan "eth0" "dhcp"
 		;;
-	glinet,gl-ar750s)
+	glinet,gl-ar750s-nor)
 		ucidef_add_switch "switch0" \
 			"0@eth0" "2:lan:2" "3:lan:1" "1:wan"
 		;;
diff --git a/target/linux/ath79/base-files/etc/hotplug.d/firmware/11-ath10k-caldata b/target/linux/ath79/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
index d93e6dcd71ab19c53905daa41e95cc4fc614f114..c917f38211d0b246f064dba4b7feefecf61f5856 100644
--- a/target/linux/ath79/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
+++ b/target/linux/ath79/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
@@ -117,7 +117,7 @@ case "$FIRMWARE" in
 		ath10kcal_extract "art" 20480 2116
 		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) +1)
 		;;
-	glinet,gl-ar750s)
+	glinet,gl-ar750s-nor)
 		ath10kcal_extract "art" 20480 2116
 		ath10kcal_patch_mac $(macaddr_add $(mtd_get_mac_binary art 0) +1)
 		;;
diff --git a/target/linux/ath79/dts/qca9563_glinet_gl-ar750s.dts b/target/linux/ath79/dts/qca9563_glinet_gl-ar750s.dts
index 03922bcd1fe9a453d5916537609317b94eea18c6..ff64e16d1ce7a94d16529e5954e1d50513a5e2cb 100644
--- a/target/linux/ath79/dts/qca9563_glinet_gl-ar750s.dts
+++ b/target/linux/ath79/dts/qca9563_glinet_gl-ar750s.dts
@@ -7,8 +7,8 @@
 #include "qca956x.dtsi"
 
 / {
-	compatible = "glinet,gl-ar750s", "qca,qca9563";
-	model = "GL.iNet GL-AR750S";
+	compatible = "glinet,gl-ar750s-nor", "qca,qca9563";
+	model = "GL.iNet GL-AR750S (NOR)";
 
 	aliases {
 		led-boot = &power;
diff --git a/target/linux/ath79/image/generic.mk b/target/linux/ath79/image/generic.mk
index 55053be34f11f0df982c85f94c9180fdba9ff221..892ef10f870e347c8a1509cecd35bce4b5e98bee 100644
--- a/target/linux/ath79/image/generic.mk
+++ b/target/linux/ath79/image/generic.mk
@@ -403,9 +403,9 @@ define Device/glinet_gl-ar750s
   DEVICE_TITLE := GL.iNet GL-AR750S
   DEVICE_PACKAGES := kmod-usb2 kmod-ath10k-ct ath10k-firmware-qca9887-ct block-mount
   IMAGE_SIZE := 16000k
-  SUPPORTED_DEVICES += gl-ar750s
+  SUPPORTED_DEVICES += gl-ar750s glinet,gl-ar750s-nor
 endef
-#TARGET_DEVICES += glinet_gl-ar750s
+TARGET_DEVICES += glinet_gl-ar750s
 
 define Device/glinet_gl-x750
   ATH_SOC := qca9531
